**FEEDER APPLICATION**

Case 1 – We use the encoder on the motor to close the position loop

Case 3 – We use the encoder located on a “free” roll to close the position loop

